M/T: Text.	Date:	08/05/2012
ON-BOARD TEST ANALYSIS RESULTS FOR LUB. OIL
Product:	Text
Equipment:	Text.	Density(at 15°C):	Text.
Quantity:	Text
SAMPLE DETAILS	Service Meter Reading	Hrs since last Oil Change	Oil added since last O/C
Text	Text	Text
VISOSITY TEST	Indication	Test Result
VISCOSITY	In the limits
By comparing fresh oil and used oil.	Outside the limits
TBN TEST	STATUS	T.B.N. (mgKOH/G)	Test Result
Satisfactory	(*)12~26 (**) 4~12
Limits are dependent on what Reagent is	Borderline	(*) 12 (**) 4
used so check the engine manufacturers	Exceeds limit	(*) < 12 (**) < 4
manual for guide lines.	(*) Limits for D/G's (12 ~ 26). (**) Limits for ME (4 ~ 12)
WATER CONTENT TEST	STATUS	% volume	Test Result
Satisfactory	(*) < 0.2 (**) < 2
Check machinery manual for limiting	Borderline	(*) = 0.2 (**) = 2
value guide lines.	Exceeds limit	(*) > 0.2 (**) > 2
(*) for engines, (**) for stern tube monitoring
SALT CONTENT TEST	Indication	Test Result
Salt Content	Yes / No	Text
SPOT TEST	Insoluble’s ---> weight % (*)
Dispersing Reserve (*)	0 - 1 %	0 - 2 %	> 2 %
Poor
Acceptable
Good
(*) - Tick a correct cell as per "LO Supplier" Manual Spot Test Interpretation Table.
Action: Text.
Responsible Officer Name:

Onboard Analysis NOT to be done in the month that the LO is sent to a 3rd party for analysis.