{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Instructions","Panasia","Techcross","Alpha Laval","Desmi"],"not_rendered":{"charts":0,"images":4,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":6,"n_cols":4,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,1,0,2]]}
[null,"SAFETY, HEALTH, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEM\n\nBALLAST WATER TREATMENT ESSENTIAL SPARES\n\nREPORTING FORMS MANUAL",null,"Form : 7.2.8\nDate : 14-Aug-2025\nRev : 10.0\nApp By : DPA"]
[]
["Please select vessel below to continue to relelvant form : "]
[]
[]
["Panasia","Techcross","Alpha Laval","Desmi"]

{"sheet":"Panasia","index":1,"n_rows":20,"n_cols":11,"rows_kept":20,"cut":false,"hidden":true,"merged":[[0,1,0,9],[4,0,4,5],[11,0,11,10],[4,6,7,6],[5,0,5,4],[6,0,6,4],[7,0,7,4]]}
[null,{"$f":"Instructions!B1","v":"SAFETY, HEALTH, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEM\n\nBALLAST WATER TREATMENT ESSENTIAL SPARES\n\nREPORTING FORMS MANUAL"},null,null,null,null,null,null,null,null,{"$f":"Instructions!D1","v":"Form : 7.2.8\nDate : 14-Aug-2025\nRev : 10.0\nApp By : DPA"}]
[]
["Vessel :","IVS Hirono",null,null,null,null,null,null,null,"Date :"]
[]
["Ballast water Treatment Essential Spares ",null,null,null,null,null,"ESSENTIAL PARTS"]
["TYPE: GloEn-P900"]
["MAKER: PANASIA"]
["FILTER UNIT "]
[null,"Component Name","Part No","MODEL / TYPE","LOCATION","Unit","Quantity","ROB","Comments","Price USD GMC ","Price USD Panasia"]
[1,"PRESSURE TRANSMITTER ---SUS316L / 0.5 Level3000 /CABLE 3m",null,"LEVEL3000","BWTS1 / RACK2 FORWARD","PC",1,null,null,800,2070]
[3,"SCANNER TIP  ----Teflon, 0.03 for suction scanner",45,"N/A","BWTS1 / RACK2 FORWARD","PC",5]
["BALLAST WATER TREATMENT SYSTEM  (FOR UV UNIT PU-250-8U)"]
[1,"UV LAMP 3.5kW ---Quartz 0.2",10,"PU3.5_1","BWTS1 / RACK2 FORWARD","PC",3,null,null,280,630]
[2,"LAMP SLEEVE ---Quartz 0.4",12,"PU3.5_1","BWTS1 / RACK2 FORWARD","PC",2]
[3,"UV INTENSITY TRANSMITTER ---(SUS316) 0.20 SUV 20.2",50,"SUV 20.2","BWTS1 / RACK2 FORWARD","PC",1,null,null,800,2070]
[4,"WIPER----For Wiper Unit",26,"N/A","BWTS1 / RACK2 FORWARD","PC",10]
[6,"QUARD-RING  ----For Lead Screw  (Ø 12.0 X Ø22.5X5t)",null,"N/A","BWTS1 / RACK2 FORWARD","PC",1]
[7,"MECHANICAL SEAL  ----For Lead Screw  ",102,"N/A","BWTS1 / RACK2 FORWARD","PC",1]
[8,"REED SWITCH  ---- For Reed Switch Housing",1,"N/A","BWTS1 / RACK2 FORWARD","PC",1]
[9,"Printer Paper for BWTS",null,null,null,"PC",1,null,null,null,40]

{"sheet":"Techcross","index":2,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":true,"merged":[[0,1,0,5],[4,0,4,6]]}
[null,{"$f":"Instructions!B1","v":"SAFETY, HEALTH, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEM\n\nBALLAST WATER TREATMENT ESSENTIAL SPARES\n\nREPORTING FORMS MANUAL"},null,null,null,null,{"$f":"Instructions!D1","v":"Form : 7.2.8\nDate : 14-Aug-2025\nRev : 10.0\nApp By : DPA"}]
[]
["Vessel :","IVS Kestrel",null,null,null,"Date :"]
[]
["Techcross Type: ECS-1000B"]
[]
["No","Component Name","Part Number","Location","Quantity","ROB","Comments"]
[3,"DC relay","YM2-LD",null,2]
[4,"AC relay","YM2-LD",null,2]
[5,"Lamp 1","YS3324 ( white)",null,2]
[6,"Lamp 2","YS3324 ( RED)",null,2]
[7,"Lamp 3","220/6V ( white)",null,2]
[8,"Lamp 4","24V ( red)",null,2]
[9,"Lamp 5","24V (green)",null,2]
[10,"Lamp 6","24V (yellow)",null,2]
[11,"Fuse","SB-C1 1A",null,4]
[12,"Fuse","FR14AM50V50 (50A/500V)",null,3]
[13,"Pru lamp","P12PSDG (GREEN)",null,1]
[14,"Pru lamp","P12PSDG (RED)",null,1]
[15,"Pru lamp","P12PSDR (WHITE)",null,1]
[16,"AC relay","SZR-MY4-N1",null,4]
[17,"Solenoid Valve","HSR130PD",null,1]
[18,"Solenoid Valve","HSR053D",null,1]
[19,"Magnetic switch","MC-100A",null,1]
[23,"CPC repair part","FUSE/CD",null,1]

{"sheet":"Alpha Laval","index":3,"n_rows":18,"n_cols":9,"rows_kept":18,"cut":false,"hidden":true,"merged":[[0,1,0,7],[4,0,4,8]]}
[null,{"$f":"Instructions!B1","v":"SAFETY, HEALTH, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEM\n\nBALLAST WATER TREATMENT ESSENTIAL SPARES\n\nREPORTING FORMS MANUAL"},null,null,null,null,null,null,{"$f":"Instructions!D1","v":"Form : 7.2.8\nDate : 14-Aug-2025\nRev : 10.0\nApp By : DPA"}]
[]
["Vessel :","IVS Okudogo",null,null,null,null,null,"Date :"]
[]
["Alfa Laval Model: CC-500 NEX"]
[]
["Stock code","Component Name","Location","Quantity","ROB","Comments","Unit Price","Total Value SGD","Global Marine Corp"]
[900952180,"UV Lamp Spare Set 6kW.",null,10,null,null,480.46,4804.6000000000004,350]
[59464582,"Quartz Sleeve Set",null,1,null,null,291.83999999999997,291.83999999999997]
[900632502,"Thermometer, Resistance\n(Replaced 900632501)",null,1,null,null,237.97,237.97]
[900632402,"Temperature Switch\n(Replaced 900632401)",null,1,null,null,155.84,155.84]
[901214601,"Lamp Power Supply.",null,2,null,null,2077.7600000000002,{"$f":"G12*2","v":4155.5200000000004}]
[900135703,"Sensor",null,1,null,null,1040.1600000000001,1040.1600000000001]
[901196392,"Maintenance  Kit",null,1,null,null,3856.45,3856.45]
[901216701,"Alpacon Descalant Offshore (Cip Liquid) -15L\n(Replaced 59625001)",null,2,null,null,142.24,284.48]
[900952180,"O Ring",null,1]
[59464582,"O Ring",null,1]
[null,null,null,null,null,null,"TOTAL COST",{"$f":"SUM(H8:H17)","v":14826.86}]

{"sheet":"Desmi","index":4,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":true,"merged":[[0,1,0,7],[4,0,4,8],[8,0,8,1]]}
[null,{"$f":"Instructions!B1","v":"SAFETY, HEALTH, ENVIRONMENT AND QUALITY MANAGEMENT SYSTEM\n\nBALLAST WATER TREATMENT ESSENTIAL SPARES\n\nREPORTING FORMS MANUAL"},null,null,null,null,null,null,{"$f":"Instructions!D1","v":"Form : 7.2.8\nDate : 14-Aug-2025\nRev : 10.0\nApp By : DPA"}]
[]
["Vessel :","IVS Kinglet",null,null,null,null,null,"Date :"]
[]
["Compact Clean Desmi Ocean Guard.Model: CC-500 NEX Cap: 500 cu.m/hr."]
[]
[null,"Component Name","Part No","Model / Type","Location","Unit","Quantity","ROB","Comments"]
[]
["Spare Part Kit Contains all the  below items:",null,441911,null,null,null,1]
[]
[1,"Seal Kit UV-Unit",441904,null,null,"PC",2]
[2,"Lamp Cup Assembly",441903,null,null,"PC",2]
[3,"Screw/Bolts Kit",441905,null,null,"PC",3]
[4,"Lamp Cable Kit",441906,null,null,"PC",2]
[5,"SP.P.KITS80-70-175/D11-02",658912,null,null,"PC",1]
[6,"AUXilitary Part Kit For ELC X12",722314,null,null,"PC",1]
[7,"Temperature Sensor",720871,null,null,"PC",1]
[8,"UV Sensor",720872,null,null,"PC",1]
[9,"UV Measurement Window G1\"",720873,null,null,"PC",1]
[10,"Centering Cyli, Ø39x3x66 PTFE",721662,null,null,"PC",4]
[11,"UV Lamp DESMI 6kW SQ",721666,null,null,"PC",2]
[12,"Quartz Tube 590x44x2.0 mm SQ",720875,null,null,"PC",2]
[13,"Pressure Transmitter",717641,null,null,"PC",1]